**LED Stage Lighting Operating Manual**

**LED 2 in1 WALL WASH Light**

**（Warm White）**





**Please Read Over This Manual before Operating the Light Fixture**

**Display description：**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Channel** | **Channel Data** | **Function instruction** |
| **1** | **CH9** | **06/09/84/89** | DMX channel mode setting |
| **2** | **d001** | **001- 512** | DMX512 address setting |
| **3** | **R255** | **000 - 255** | 3in1 red dimmer |
| **4** | **G255** | **000 - 255** | 3in1 green dimmer |
| **5** | **B255** | **000 - 255** | 3in1 blue dimmer |
| **6** | **H255** | **000 - 255** | Single Warm White dimmer |
| **7** | **Pr01** | **1 - 30** | Preset effect |
| **8** | **SP16** | **00 - 20** | Speed setting |
| **9** | **Auto** | **Auto/Audi** | Testing mode, switching between auto run and sound by pressing button A/B |
| **10** | **DISP** | **/** | Display setting |

**DMX Channel description**

**6 Channel Mode**

|  |  |  |
| --- | --- | --- |
| **CH** | **function** | **instruction** |
| CH1 | 000-255 | Dimmer |
| CH2 | 000-255 | Strobe |
| CH3 | 000-255 | 3in1 R red dimmer |
| CH4 | 000-255 | 3in1G green dimmer |
| CH5 | 000-255 | 3in1B blue dimmer |
| CH6 | 000-255 | Warm white dimmer |

**9 Channel Mode**

|  |  |  |
| --- | --- | --- |
| **CH** | **function** | **instruction** |
| CH1 | 000-255 | Dimmer |
| CH2 | 005-255 | Strobe |
| CH3 | 000-255 | 3in1 R red dimmer |
| CH4 | 000-255 | 3in1G green dimmer |
| CH5 | 000-255 | 3in1B blue dimmer |
| CH6 | 000-255 | Warm white dimmer |
| CH7 | 001-255 | Color mixing |
| CH8 | 001-255 | Preset effect selection |
| CH9 | 000-255 | speed |

**84 Channel Mode**

|  |  |  |
| --- | --- | --- |
| **CH** | **function** | **instruction** |
| CH1 | 000-255 | W1 Warm white dimmer |
| CH2 | 005-255 | W2 Warm white dimmer |
| ... | ... ... | ...... |
| CH11 | 006-255 | W11 Warm white dimmer |
| CH12 | 000-255 | W12 Warm white dimmer |
| CH13 | 000-255 | 1# 3in1 R red dimmer |
| CH14 | 000-255 | 1# 3in1G green dimmer |
| CH15 | 000-255 | 1# 3in1B blue dimmer |
| CH16 | 000-255 | 2# 3in1 R red dimmer |
| CH17 | 000-255 | 2# 3in1G green dimmer |
| CH18 | 000-255 | 2# 3in1B blue dimmer |
| ... | ...... |  |
| CH82 | 000-255 | 24# 3in1 R red dimmer |
| CH83 | 000-255 | 24# 3in1G green dimmer |
| CH84 | 000-255 | 24# 3in1B blue dimmer |

|  |  |  |
| --- | --- | --- |
| **CH** | **function** | **instruction** |
| CH1 | 000-255 | dimmer |
| CH2 | 005-255 | strobe |
| CH3 | 000-255 | W1 Warm white dimmer |
| CH4 | 005-255 | W2 Warm white dimmer |
| ... | ... ... | ...... |
| CH13 | 006-255 | W11 Warm white dimmer |
| CH14 | 000-255 | W12 Warm white dimmer |
| CH15 | 000-255 | 1# 3in1 R red dimmer |
| CH16 | 000-255 | 1# 3in1G green dimmer |
| CH17 | 000-255 | 1# 3in1B blue dimmer |
| CH18 | 000-255 | 2# 3in1 R red dimmer |
| CH19 | 000-255 | 2# 3in1G green dimmer |
| CH20 | 000-255 | 2# 3in1B blue dimmer |
| ... | ...... |  |
| CH84 | 000-255 | 24# 3in1 R red dimmer |
| CH85 | 000-255 | 24# 3in1G green dimmer |
| CH86 | 000-255 | 24# 3in1B blue dimmer |
| CH87 | 001-255 | Color mixing |
| CH88 | 001-255 | Preset effect selection |
| CH89 | 000-255 | speed |

**89 Channel Mode**